create_item("mr_tube_triode","Verilog-A implementation of Triode","T",0,-1,NULL,"Component Parameters",NULL,"%0b\"%p\"%1e:%t %# %44?0%:%31?%C%:_net%c%;%;%e %1b%r%8?%29?%:%30?%p %:%k%?[%1i]%;=%p %;%;%;%e%e","","%t%b%r%38?%:\n%30?%s%:%k%?[%1i]%;=%s%;%;%e%e%;","",0,NULL,32,
create_parm("Model","Model instance name",0,"StdFileFormSet",-1,prm("StdForm","mr_triode")),
create_parm("Kp","Perveance of the triode",3584,"StdFileFormSet",-1,prm("StdForm","")),
create_parm("smallKp","Fitting parameter",3584,"StdFileFormSet",-1,prm("StdForm","")),
create_parm("kvb","fitting parameter",3584,"StdFileFormSet",-1,prm("StdForm","")),
create_parm("mu","amplification factor",3584,"StdFileFormSet",-1,prm("StdForm","")),
create_parm("X","Fitting parameter",3584,"StdFileFormSet",-1,prm("StdForm","")),
create_parm("cgc","Grid-Cathode capacitance",3584,"StdFileFormSet",4,prm("StdForm","")),
create_parm("cga","Grid-Anode capacitance",3584,"StdFileFormSet",4,prm("StdForm","")),
create_parm("cac","Anode-Cathode capacitance",3584,"StdFileFormSet",4,prm("StdForm","")),
create_parm("Tchatode","Cathode temperature (noise analysis only)",3584,"StdFileFormSet",12,prm("StdForm","")),
create_parm("gm","Transconductance (noise analysis only)",3584,"StdFileFormSet",-1,prm("StdForm","")));
