create_constant_form("on","ON",0,"1","on");
create_constant_form("off","OFF",0,"0","off");
create_form_set("RegionFormSet","on","off");

create_constant_form("linear","Linear",0,"0","linear");
create_constant_form("nonlinear","Nonlinear",0,"1","nonlinear");
create_form_set("ModeFormSet","linear","nonlinear");

create_constant_form("yes","YES",0,"yes","yes");
create_constant_form("no","NO",0,"no","no");
create_form_set("NoiseFormSet","yes","no");

create_item("mr_diode_zener","mr_diode_zener","D",0,-1,NULL,"Component Parameters",NULL,"%0b\"%p\"%1e:%t %# %44?0%:%31?%C%:_net%c%;%;%e %1b%r%8?%29?%:%30?%p %:%k%?[%1i]%;=%p %;%;%;%e%e","","%t%b%r%38?%:\n%30?%s%:%k%?[%1i]%;=%s%;%;%e%e%;","",0,NULL,32,
create_parm("Model","Model instance name",0,"StdFileFormSet",-1,prm("StdForm","")),
create_parm("Temp","Temperature",7680,"StdFileFormSet",12,prm("StdForm","")),
create_parm("Trise","Temperature rise over ambient",7680,"StdFileFormSet",12,prm("StdForm","")),
create_parm("Region","DC operating region, (default: ON)",544,"RegionFormSet",-1,prm("on")),
create_parm("Mode","Simulation mode, (default: nonlinear)",544,"ModeFormSet",-1,prm("nonlinear")),
create_parm("Noise","Temperature coefficient; per degree Celsius squared",544,"NoiseFormSet",-1,prm("yes")),
create_parm("_M","Number of devices in parallel, (default: 1)",512,"StdFileFormSet",-1,prm("StdForm","1")));
